

Safety Data Sheet Dynaflux SDS 390A 07/18/2018

Product: 390 Non-Toxic Anti-Spatter (Aerosol)

**Part 1: Product and Company Identification**

Identification 390A

Trade Name: 390 Non-Toxic Anti-Spatter

Product Use: Non-Solvent Anti-Spatter.

Manufacturers Name: Dynaflux, Inc.

241 Brown Farm Rd.

Cartersville, GA 30120 U.S.A.

Emergency Telephone Number: For U.S.: 800-255-3924 International: 813-248-0585

**Part 2: Hazard(s) Identification**

Contains No Hazardous Ingredients at or above 1%.



Signal Word:  **WARNING**

**H229:** Pressurized container: may burst if heated

**Part 3: Composition / information on ingredients**

**Emergency Overview:**

Caution: Contents Under Pressure.

Aerosol: Do not puncture or incinerate. Do not expose to heat or store at temperatures above 120°F.

Primary route(s) of entry. Skin and eye contact. Inhalation.

Eyes: May cause temporary irritation.

Skin: Prolonged skin contact may cause drying and defatting of skin.

Inhalation: My irritate mucosal tissue.

Ingestion: Not a like route of exposure (aerosol). Ingestion may result in nausea, abdominal discomfort or diarrhea.

Potential Chronic Health Effects: None

Carcinogenic Effects:

NTP: No

IARC: No

OSHA: No

ACGIH: No

Mutagenic Effects: None

Teratogenic Effects: None

Target Organs: None

Medical Conditions Aggravated by Exposure: None

May cause allergic reaction in individuals who are allergic to soy.

Signs and Conditions: Stinging in eyes. Repeated or prolonged skin contact can cause redness, irritation and scaling if the skin (dermatitis).

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **H.M.I.S.** |  | |  | | **N.F.P.A.** | |  |
| Health | 1 | |  | | Health | | 1 |
| Flammability | 0 | |  | | Flammability | | 0 |
| Reactivity | 0 | |  | | Reactivity | | 0 |
| Special | B | |  | | Personal Protection | | - |
|  | |  | |  | |  | | |  |

**Part 4: First Aid Measures**

Eyes: Flush eyes with cool, clean water (low pressure) for at least 15 minutes. Hold eyelids apart to ensure complete irrigation of

the eye and eyelid. If irritation persists seek medical attention.

Skin: Should irritation occur wash affected area with soap and water for 15 minutes. Lauder clothing before reuse. If irritation

persists seek medical attention.

Inhalation: No irritation with inhalation should occur. Remove to fresh air. If not breathing give artificial respiration. Seek

medical attention.

Ingestion: Ingestion is unlikely. Should ingestion occur, do not induce vomiting unless directed to do so by medical personnel.

Drink a glass of water or milk to dilute. Never give anything by mouth to an unconscious person. Seek medical attention

immediately.

**Part 5: Fire Fighting Measures**

Flashpoint: Nonflammable Flame Projection Test

U.E.L.: None Established

L.E.L. : None Established

Auto Ignition Temperature: NA

Combustion Products: Carbon dioxide, carbon monoxide.

Extinguishing Media: Foam, CO2, Dry chemical

Unusual Fire and Explosion Hazard: Use a self- contained breathing apparatus. Use water fog to cool containers to prevent rupturing of containers. Aerosols may explode upon heating, spread fire and overcome sprinkler systems.

**Part 6: Accidental Release Measures**

Small Spill: Soak up with absorbent material, i.e. kitty litter, clay or dirt. Sweep up and place in a labeled closed container.

Large Spill: Keep unauthorized people from the area. Dike area and pump contents to a labeled, closed container. Absorb residue and sweep up. Place in a closed, labeled container. Dispose of properly.

**Part 7: Handling and Storage**

Leave in the shipping containers. Store in a cool dry place. Do not expose aerosols to temperatures above 120° F or the container may rupture. Store aerosol as Level 1 Aerosol (NFPA 30B).

**Part 8: Exposure Control / Personal Protection**

Personal Protection:

Eye: Safety Glasses with side shields conforming to appropriate regulations.

Hand Protection: None required. Use of chemically resistant gloves is recommended.

Respiratory Protection: Use of this product as per label instructions does not require the use of respiratory protection. If airborne concentrations are above the applicable exposure limits use NIOSH approved respiratory protection (organic vapor cartridge).

Continued next page

**Part 9: Physical and Chemical Properties**

Boiling Point: 212°F (100 C)

Vapor Pressure :

(PSIG @ 70°F): 120 psig

Vapor Density (Air=1): .62

Appearance and Odor: Light amber liquid with no odor.

Specific Gravity: (H2O)=1): .97mmHg

Evaporation Rate (H2O=1): 1

Water Reactive: No

Solubility in water: Miscible

Flash Point: None

Decomposition Temperature: Not Established

**Part 9: Physical and Chemical Properties: (Continued):**

Auto Ignition Temperature: Not Established

Flammable Limits:

Lower: Not Established

Upper: Not Established

Partition Coefficient: (Octanol/Water): <1

VOC Content: .5% (by weight)

**Part 10: Stability and Reactivity**

Stability- Product is stable

Hazardous Polymerization- will not occur.

Avoid extreme heat and freezing.

**Part 11: Toxicological Information**

An acute toxicity study of this product has not been conducted. Information given in this section relates only to individual constituents contained in this compound.

**Part 12: Ecological Information**

Mobility: Low volatility. Will Absorb into soil.

Persistence and Degradability: 100% Biodegradable / Inert.

Bioaccumulative Potential: no bioaccumulation potential.

Other adverse effects: None

**Part 13: Disposal Consideration**

Waste must be disposed of in accordance with national, regional, provincial, state and local environmental control regulations.

Do not dump into any sewers, on the ground or into any body of water.

**Part 14: Transportation Information**

**DOT HM-181 Shipping Information**

D.O.T. Shipping Name – Consumer Commodity

Hazard Class or Division: ORM-D (on shipping carton)

UN Number: NA

Packing Group: None

Label(s) Required: ORM-D (on shipping carton)

Continued next page

**IMDG-IMO:**

UN No. : 1950

Class: 2

Shipping Name: Aerosols

Subsidiary Risk: 2.2

Labeling: Non-Flammable Gas

Packing Group: III

EMS: F-D, S-U

Marine Pollutant: NO

Technical Name: NA

**Part 15: Regulatory Information**

CERCLA: None

TSCA: All components of this product are TSCA Inventory Listed and/or are exempt.

SARA TITLE III SARA Section 311 and 312 (40 CFR 370) Hazard Categories: Sudden Release of Pressure.

State Regulations:

California Proposition 65

This product does not contain chemical(s) known to the State of California to cause cancer, birth defects or reproductive harm.

California and OTC States:

This product is not regulated by Consumer Regulations.

Canadian Environmental Protection Act:

All of the components of this product are included on the Canadian Domestic Substances List (DSL).

Canadian Workplace Hazardous Materials Information System: WHMIS

This product has been classified in accordance with the hazard criteria of the controlled products regulations and the MSDS contains all the information required by the controlled products regulations.

WHMIS Classification: Aerosol: Class A, Class D2B

A Compressed Gas

D2 Materials causing other toxic effects.

Montreal Protocol Listed Ingredient: None

Stockholm Convention Listed Ingredient: None

Rotterdam Convention Listed Ingredients: None

ROHS Compliant: Yes

**Part 16: Other Information**

Responsible Name: Gene Schaffstall

Senior Chemist

Telephone: 1-800-334-4420 or (770)-382-8843

**Disclaimer of Expressed and implied Warranties:**

The information presented in this Safety Data Sheet is based on data believed to be accurate as of the date of the l Safety Data sheet was prepared. No responsibility is assumed for any damage or injury resulting from abnormal use or from any failure to adhere to recommended practices as specified on the label copy.